NFS-Root Mini-Howto

Table of Contents

NFS-Root Mini-Howto ......................................................................................................................................1 Andreas Kostyrka, andreas@ag.or.at.......................................................................................................1 1. Copyright.............................................................................................................................................1 2. General Overview................................................................................................................................1 3. Setup on the server...............................................................................................................................1 4. Booting the workstation.......................................................................................................................1 5. Known problems..................................................................................................................................1 6. Other topics..........................................................................................................................................1 1. Copyright.............................................................................................................................................1 1.1 Contributors.......................................................................................................................................2 2. General Overview................................................................................................................................2 3. Setup on the server...............................................................................................................................3 3.1 Compiling the kernels........................................................................................................................3 3.2 Creation of the root filesystem...........................................................................................................3 Copying the filesystem...............................................................................................................3 Changes to the root filesystem....................................................................................................3 Exporting the filesystem.............................................................................................................4 RARP setup.................................................................................................................................4 BOOTP setup..............................................................................................................................4 Finding out hardware addresses..................................................................................................4 4. Booting the workstation.......................................................................................................................5 4.1 Using a boot rom................................................................................................................................5 4.2 Using a raw kernel disc......................................................................................................................5 4.3 Using a bootloader & RARP.............................................................................................................5 4.4 Using a bootloader without RARP....................................................................................................5 5. Known problems..................................................................................................................................6 5.1 /sbin/init doesn'tstart.........................................................................................................................6 5.2 /dev troubles......................................................................................................................................6 6. Other topics..........................................................................................................................................6

i

NFS-Root Mini-Howto

Andreas Kostyrka, andreas@ag.or.at

V8, 8 August 1997

This Mini-HOWTO tries explains how to setup a ``disc-less'' Linux workstation, which mounts it's root filesystems via NFS. The newest version of this Mini-Howto can always be found in

ftp://sunsite.unc.edu/pub/Linux/docs/HOWTO/mini/NFS-Root or on any sunsite mirror

NEAR YOU.

1. Copyright

1.1 Contributors • 2. General Overview

3. Setup on the server

3.1 Compiling the kernels • 3.2 Creation of the root filesystem • 4. Booting the workstation

4.1 Using a boot rom • 4.2 Using a raw kernel disc • 4.3 Using a bootloader & RARP • 4.4 Using a bootloader without RARP • 5. Known problems

5.1 /sbin/init doesn't start. • 5.2 /dev troubles. • 6. Other topics

1. Copyright

(c) 1996 Andreas Kostyrka (e9207884@student.tuwien.ac.at or andreas@ag.or.at)

Unless otherwise stated, Linux HOWTO documents are copyrighted by their respective authors. Linux HOWTO documents may be reproduced and distributed in whole or in part, in any medium physical or

NFS-Root Mini-Howto 1 electronic, as long as this copyright notice is retained on all copies. Commercial redistribution is allowed and encouraged; however, the author would like to be notified of any such distributions.

All translations, derivative works, or aggregate works incorporating any Linux HOWTO documents must be covered under this copyright notice. That is, you may not produce a derivative work from a HOWTO and impose additional restrictions on its distribution. Exceptions to these rules may be granted under certain conditions; please contact the Linux HOWTO coordinator at the address given below.

In short, we wish to promote dissemination of this information through as many channels as possible. However, we do wish to retain copyright on the HOWTO documents, and would like to be notified of any plans to redistribute the HOWTOs.

If you have questions, please contact Andreas Kostyrka <mailto:andreas@ag.or.at>, the author of this mini-HOWTO, or Tim Bynum, the Linux HOWTO coordinator, at <mailto:linux-howto@sunsite.unc.edu> via email.

1.1 Contributors

Avery Pennarun <apenwarr@foxnet.net> (how to boot without LILO) • Ofer Maor <ofer@hadar.co.il> (providing a better mini howto about setting up discless workstations.) • Christian Leutloff <leutloff@sundancer.tng.oche.de> (providing infos about netboot.) • 2. General Overview

Generally speaking there are the following problems for the workstation:

It must find out it's own IP-address, and if needed also the rest of the Ethernet configuration. • It must know the NFS-server and the mount path to it's root filesystem. • The current implementation of NFSROOT in the Linux kernel (as of 1.3.7x) allows for the following ``solutions'':

The IP-address may be discovered by RARP, or the full ethernet configuration may be passed to the kernel via kernel parameters by LILO or LOADLIN. • The NFS-path to mount can be passed via kernel parameters. If this is not done, the kernel assumes the RARP-server also as NFS-server, and uses compiled in default for the path part. (current default value in the kernel: /tftpboot/<IP-address of the machine>.) •

The client configuration may be discovered by BOOTP. • Before starting to setup a discless enviroment, you should decide if you will be booting via LILO or LOADLIN. The advantage of doing so is flexibility, the disadvantage is speed. Booting a Linux kernel without LILO is faster. This may or may not be a consideration.

1.1 Contributors 2

3. Setup on the server

3.1 Compiling the kernels

RARP support in the kernel of the server will probably be a good idea. You must have it if you will boot without kernel parameters. On the other hand it doesn't help you, if the client isn't on the same subnet than the server.

The kernel for the workstation needs the following as a minimum set compiled in:

NFS-filesystem compiled in. (It doesn't need to have ext2-support compiled in, a module suffices.) • ``Root on NFS'' must be enabled. • The Ethernet driver for the network card of the workstation must be compiled in. • Depending upon your needs you may have to include RARP or BOOTBP support for NFS-Root. (By this I mean the questions that are asked after the NFS question in make config.) •

If the workstation will be booted without kernel parameters, you need also to set the root device to 0:255. Do this by creating a dummy device file with mknod /dev/nfsroot b 0 255. After having created such a device file, you can set root device of the kernel image with rdev <kernel-image> /dev/nfsroot.

3.2 Creation of the root filesystem

Copying the filesystem

Warning: while these instruction might work for you, they are by no means sensefull in a production enviroment. For a better way to setup a root filesystem for the clients, see the NFS-Root-Client mini howto by Ofer Maor <ofer@hadar.co.il>.

After having decided where to place the root tree, create it with (e.g.) mkdir -p <directory> and

tar cClf / - | tar xpCf <directory> -.

If you boot your kernel without LILO, then the rootdir has to be /tftpboot/<IP-address>. If you don't like it, you can change it in the top Makefile in the kernel sources, look for a line like: NFS_ROOT =

-DNFS_ROOT="\"/tftpboot/%s\"" If you change this, you have to recompile the kernel.

Changes to the root filesystem

Now trim the unneeded files, and check the /etc/rc.d scripts. Some important points:

One important thing is eth0 setup. The workstation comes up with a, at least partially, setup eth0. Setting up the IP-address of the workstation to the the IP-Address of the server is not considered a clever thing to do. (As it happened to the author on one of his early attempts.) •

Another point is the /etc/fstab of the workstation. It should be setup for nfs filesystems. • WARNING: Don't confuse the server root filesystem and the workstation root filesystem. (I've already patched up a rc.inet1 on the server, and wondered why the workstation still didn't work.) •

3. Setup on the server 3

Exporting the filesystem

Export the root dir to the work station. See exports(5). You most likely will have to restart the nfsd/mountd after this change. Under RedHat this can easily be done by typing

/etc/rc.d/init.d/nfs stop ; /etc/rc.d/init.d/nfs start .

RARP setup

Setup the RARP somewhere on the net. If you boot without a nfsroot parameter, the RARP server has to be the NFS server. Usually this will be the NFS server. To do this, you will need to run a kernel with RARP support. To do this, execute (and install it somewhere in /etc/rc.d of the server!):

/sbin/rarp -s <ip-addr> <hardware-addr>

where ip-addr

is the IP address of the workstation, and hardware-addr

is the Ethernet address of the network card of the workstation. example: /sbin/rarp -s 131.131.90.200 00:00:c0:47:10:12 You can also use a symbolic name instead of the IP-address, as long the server is able to find out the IP-address. (/etc/hosts or DNS lookups)

BOOTP setup

For BOOTP setup you need to edit /etc/bootptab. Please consult the bootpd(8) and bootptab(5) man pages.

Finding out hardware addresses

I don't know the hardware address! How can I find it out?

Boot the kernel disk you made, and watch for the line where the network card is recognized. It usually contains 6 hex bytes, that should be the address of the card. • Boot the workstation with some OS with TCP/IP networking enabled. Then ping the workstation from the server. Look in the ARP-cache by executing: /sbin/arp -a •

Exporting the filesystem 4

4. Booting the workstation

4.1 Using a boot rom

As I have not used such a beast myself yet, I can give you only the following tips (courtesy of Christian Leutloff <leutloff@sundancer.tng.oche.de>):

You can't use ``normal'' bootroms. • There is a netboot packet by Gero Kuhlmann, that provides for bootroms for Linux, and further information. netboot is available from the local Linux mirror, or as a Debian package (netboot-0.4). •

Read the documentation coming with your boot rom carefully. • You probably will have to enable the tftpd on the server, but this depends upon your boot rom's way of loading the kernel. • Any informations on bootrom vendors of these Linux variety, mentioned above, as not everybody has access to prom burner :( (especially in europe, as I'm located there.) welcome, I'll include them then here. •

4.2 Using a raw kernel disc

If you have exported the root filesystem with the correct name for the default naming and your NFS server is also the RARP server (which implies that the boxes are on the same subnet.), than you can just boot the kernel by cating it to a disc. (You have to set the root device in the kernel to 0:255.) This assumes, that the root directory on the server is /tftpboot/IP-Address (this value can be changed when compiling the kernel.)

4.3 Using a bootloader & RARP

Give the kernel all needed parameters when booting, and add

nfsroot=<server-ip-addr>:</path/to/mount> where server-ip-addr is the IP-address of

your NFS-server, and /path/to/mount is the path to the root directory.

Tips:

When using LILO consider using the ``lock'' feature: Simply type in once all the correct parameters and add ``lock''. Next time when booting let LILO timeout. • When generating a workstation specific boot disk, you can also use the append= feature in

lilo.conf.

• 4.4 Using a bootloader without RARP

In addition to nfsroot give a

nfsaddrs=<wst-IP>:<srv-IP>:<gw-IP>:<netm-IP>:<hostname> commandline argument

for the kernel. The kernel will setup eth0 with the given parameters:

wst-IP

machine's IP-Address

4. Booting the workstation 5 srv-IP

NFS-server IP-Address

gw-IP

gateway

netm-IP

netmask

hostname

machine name

5. Known problems

5.1 /sbin/init doesn't start.

A popular problem with /sbin/init is, that some (at least) current distributions come with /sbin/init dynamically linked. So you have to provide a correct /lib setup to the client. One easy thing one could try is replacing /sbin/init (for the client) with a statically linked ``Hello World'' program. This way you know if it is something more basic, or ``just'' a problem with dynamic linking.

5.2 /dev troubles.

If you get some garbled messages about ttys when booting, then you should run a MAKEDEV from the client in the /dev directory. There are rumors that this doesn't work with certain server oses which use 64-bit dev numbers, should you run into this, please mail me with which os you have the troubles. A potential solution would be to create a small /dev ram disc early in the boot process, and reinstall the device nodes each time.

6. Other topics

There is BOOTP client:

ftp://sunsite.unc.edu/system/Network/admin/bootpc.v045.tgz

•

With initrd (which is included in Linux 2.0), it could be made to work for diskless stations quite nicely. initrd is actually always an advanced option for more customized setups.

For plain bootpd based boots this is actually probably not needed as Linux 2.0 contains also the option to use BOOTP instead of RARP. (To be more precise, you can compile both in the kernel, and the faster response wins.) •

In the Documentation directory of kernel source there is a file documenting NFS-Root systems. • There is a patch floating around, that allows for swapping over NFS. It was send to me (during a private high workload phase), but I somehow managed to loose the mail. :( •

You can get it probably from http://www.linuxhq.com/ in the unofficial patches section. My PGP public key can be fetched by fingering andreas@ag.or.at. The fingerprint is: F1 F7 43 D5 07 C4 6C 87 BF 6B 33 A2 2C EE 5A F9. •